                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:1287376
Raspberry Pi B+ and 7" Display Stand by maddavo is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

This is a case and stand for the Raspberry Pi B+ and 7" Touch screen display.  The stand has an adjustable angle.

### Hardware:###
1x Raspberry Pi B+
1x 7" Touch Screen & Display board (I got mine from Element14 at http://au.element14.com/webapp/wcs/stores/servlet/ProductDisplay?catalogId=15001&langId=43&urlRequestType=Base&partNumber=247387201&storeId=10184)
1x M4x16 screw
1x M4 nut
4x M3x8 screws
2x M3x10 self-tapping screws

### Instructions:###
1. Attach the cover to the back of the Pi/Display using the 4 M3x8 screws - ensure that the cables are all comfortably tucked in.
2. Attach the bezel to the front of the Pi/Display by inserting the top of the display into the top of the bezel and then lock into position using 2 M3x10 self-tapping screws.
3. Insert the M4 nut into the back of the cover, insert the M4 screw into the bottom of the base so it pokes out the top, then screw together.

This is probably best printed in PLA unless you are good at keeping your ABS from warping.  There are some pretty fine tolerances involved.

Enjoy!

### Changelog: ###

23/1/2016: Updated Rear.STL - M4 nut cavity was too small.
24/1/2016: Updated Rear.STL - moved some holes for connectors.
26/1/2016:  Test print successful for Rear.STL and Stand.STL .  Now printing Bezel to complete test.
28/1/2016:  Test print successful - all the parts seem to fit together OK.

### To do: ###
Future revisions may include the following:
* Add hole for camera ribbon cable
* Add mount for camera board
* Add HDMI port and mounting for https://www.tindie.com/products/freto/pi-camera-hdmi-cable-extension/