Arduino A2DP

BluetoothA2DPSinkMinRAM Member List

This is the complete list of members for BluetoothA2DPSinkMinRAM, including all inherited members.

activate_pin_code(bool active) | BluetoothA2DPSink | virtual
address_validator (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
app_a2d_callback(esp_a2d_cb_event_t event, esp_a2d_cb_param_t *param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_alloc_meta_buffer(esp_avrc_ct_cb_param_t *param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_gap_callback(esp_bt_gap_cb_event_t event, esp_bt_gap_cb_param_t *param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_rc_ct_callback(esp_avrc_ct_cb_event_t event, esp_avrc_ct_cb_param_t *param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_send_msg(app_msg_t *msg) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_task_handle (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
app_task_handler(void *arg) | BluetoothA2DPSink | protected virtual
app_task_queue (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
app_task_shut_down(void) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_task_start_up(void) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_work_dispatch(app_callback_t p_cback, uint16_t event, void *p_params, int param_len) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
app_work_dispatched(app_msg_t *msg) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
audio_data_callback(const uint8_t *data, uint32_t len) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
audio_state (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
audio_state_callback (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
audio_state_obj (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
audio_type (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
av_hdl_a2d_evt(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
av_hdl_avrc_evt(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
av_hdl_stack_evt(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
av_new_track() (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
av_notify_evt_handler(uint8_t event_id, uint32_t event_parameter) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
avrc_metadata_callback (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
avrc_metadata_flags (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
BluetoothA2DPSink() | BluetoothA2DPSink |
BluetoothA2DPSinkMinRAM()=default (defined in BluetoothA2DPSinkMinRAM) | BluetoothA2DPSinkMinRAM |
bt_connected (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
bt_dis_connected (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
bt_i2s_task_shut_down(void) override (defined in BluetoothA2DPSinkMinRAM) | BluetoothA2DPSinkMinRAM | inline virtual
bt_i2s_task_start_up(void) override (defined in BluetoothA2DPSinkMinRAM) | BluetoothA2DPSinkMinRAM | inline virtual
bt_name (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
bt_volumechange (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
clean_last_connection() (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
confirm_pin_code() | BluetoothA2DPSink | virtual
confirm_pin_code(int code) | BluetoothA2DPSink | virtual
connect_to_last_device() (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
connection_rety_count (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
connection_state (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
connection_state_callback (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
connection_state_obj (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
data_received (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
debounce(void(*cb)(void), int ms) | BluetoothA2DPCommon | virtual
debounce_ms (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
default_volume_control (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
disconnect() | BluetoothA2DPCommon | virtual
end(bool release_memory=false) | BluetoothA2DPSink | virtual
end_in_progress (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
esp_spp_mode (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected static
event_queue_size (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
event_stack_size (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
execute_avrc_command(int cmd) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
fast_forward() | BluetoothA2DPSink | virtual
get_audio_state() | BluetoothA2DPCommon | virtual
get_audio_type() | BluetoothA2DPSink | virtual
get_connection_state() | BluetoothA2DPCommon | virtual
get_current_peer_address() | BluetoothA2DPSink | inline virtual
get_last_connection() (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
get_last_peer_address() | BluetoothA2DPCommon | inline virtual
get_last_rssi() | BluetoothA2DPSink | inline
get_volume() | BluetoothA2DPSink | virtual
handle_audio_cfg(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
handle_audio_state(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
handle_connection_state(uint16_t event, void *p_param) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
has_last_connection() (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
i2s_channels (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_config (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_mclk_pin_select(const uint8_t pin) | BluetoothA2DPSink | virtual
i2s_port (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_ringbuffer_size (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_stack_size (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_task_handler(void *arg) override (defined in BluetoothA2DPSinkMinRAM) | BluetoothA2DPSinkMinRAM | inline virtual
i2s_task_priority (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
i2s_write_data(const uint8_t *data, size_t item_size) | BluetoothA2DPSink | protected
init_bluetooth() (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
init_i2s() (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
init_nvs() (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected virtual
is_auto_reconnect (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
is_connected() | BluetoothA2DPSink | virtual
is_connecting (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
is_i2s_output (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
is_pin_code_active (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
is_reconnect(esp_a2d_disc_rsn_t type) (defined in BluetoothA2DPSink) | BluetoothA2DPSink | inline protected virtual
is_start_disabled (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
is_volume_used (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
last_bda_nvs_name() (defined in BluetoothA2DPSink) | BluetoothA2DPSink | inline protected virtual
last_connection (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
last_rssi_delta (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
log_free_heap() | BluetoothA2DPCommon |
m_a2d_audio_state_str (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
m_a2d_conn_state_str (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
m_pkt_cnt (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
next() | BluetoothA2DPSink | virtual
pause() | BluetoothA2DPSink | virtual
peer_bd_addr (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
pin_code() | BluetoothA2DPSink | inline virtual
pin_code_int (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
pin_code_request (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
pin_code_str (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
pin_config (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
play() | BluetoothA2DPSink | virtual
player_init (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
previous() | BluetoothA2DPSink | virtual
reconnect() | BluetoothA2DPCommon | inline virtual
reconnect_on_normal_disconnect (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
rewind() | BluetoothA2DPSink | virtual
rssi_active (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
rssi_callbak (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
s_bt_i2s_task_handle (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
s_ringbuf_i2s (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
s_volume (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
s_volume_lock (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
s_volume_notify (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
sample_rate() | BluetoothA2DPSink | virtual
sample_rate_callback (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
set_address_validator(bool(*callBack)(esp_bd_addr_t remote_bda)) | BluetoothA2DPSink | inline virtual
set_auto_reconnect(bool reconnect, bool afterNormalDisconnect=false, int count=AUTOCONNECT_TRY_NUM) | BluetoothA2DPSink | inline virtual
BluetoothA2DPCommon::set_auto_reconnect(bool active) | BluetoothA2DPCommon | inline
set_avrc_metadata_attribute_mask(int flags) | BluetoothA2DPSink | inline virtual
set_avrc_metadata_callback(void(*callback)(uint8_t, const uint8_t *)) | BluetoothA2DPSink | inline virtual
set_bits_per_sample(int bps) | BluetoothA2DPSink | inline virtual
set_channels(i2s_channel_t channels) | BluetoothA2DPSink | inline virtual
set_connected(bool active) | BluetoothA2DPCommon | inline virtual
set_event_queue_size(int size) | BluetoothA2DPSink | inline
set_event_stack_size(int size) | BluetoothA2DPSink | inline
set_i2s_config(i2s_config_t i2s_config) | BluetoothA2DPSink | virtual
set_i2s_port(i2s_port_t i2s_num) | BluetoothA2DPSink | virtual
set_i2s_ringbuffer_size(int size) | BluetoothA2DPSink | inline
set_i2s_stack_size(int size) | BluetoothA2DPSink | inline
set_i2s_task_priority(UBaseType_t prio) | BluetoothA2DPSink | inline
set_last_connection(esp_bd_addr_t bda) (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
set_mono_downmix(bool enabled) | BluetoothA2DPSink | inline virtual
set_on_audio_state_changed(void(*callBack)(esp_a2d_audio_state_t state, void *), void *obj=nullptr) | BluetoothA2DPCommon | virtual
set_on_connection_state_changed(void(*callBack)(esp_a2d_connection_state_t state, void *), void *obj=nullptr) | BluetoothA2DPCommon | virtual
set_on_data_received(void(*callBack)()) | BluetoothA2DPSink | virtual
set_on_volumechange(void(*callBack)(int)) | BluetoothA2DPSink | virtual
set_pin_config(i2s_pin_config_t pin_config) | BluetoothA2DPSink | virtual
set_rssi_active(bool active) | BluetoothA2DPSink | inline
set_rssi_callback(void(*callback)(esp_bt_gap_cb_param_t::read_rssi_delta_param &rssi)) | BluetoothA2DPSink | inline
set_sample_rate_callback(void(*callback)(uint16_t rate)) | BluetoothA2DPSink | inline virtual
set_scan_mode_connectable(bool connectable) (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected virtual
set_stream_reader(void(*callBack)(const uint8_t *, uint32_t), bool i2s_output=true) | BluetoothA2DPSink | virtual
set_swap_lr_channels(bool swap) | BluetoothA2DPSink | inline virtual
set_task_priority(UBaseType_t priority) | BluetoothA2DPCommon | inline
set_volume(uint8_t volume) | BluetoothA2DPSink | virtual
set_volume_control(A2DPVolumeControl *ptr) | BluetoothA2DPCommon | inline virtual
start(const char *name, bool auto_reconect) | BluetoothA2DPSink | virtual
start(const char *name) | BluetoothA2DPSink | virtual
stop() | BluetoothA2DPSink | virtual
stream_reader (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
swap_left_right (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
task_priority (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
to_str(esp_a2d_connection_state_t state) | BluetoothA2DPCommon |
to_str(esp_a2d_audio_state_t state) | BluetoothA2DPCommon |
to_str(esp_bd_addr_t bda) | BluetoothA2DPCommon |
try_reconnect_max_count (defined in BluetoothA2DPSink) | BluetoothA2DPSink | protected
volume_control() | BluetoothA2DPCommon | inline protected virtual
volume_control_ptr (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
volume_value (defined in BluetoothA2DPCommon) | BluetoothA2DPCommon | protected
write_ringbuf(const uint8_t *data, size_t size) | BluetoothA2DPSinkMinRAM | inline virtual
~BluetoothA2DPCommon()=default | BluetoothA2DPCommon | virtual
~BluetoothA2DPSink() | BluetoothA2DPSink | virtual